1. **نظام مراقبة وإدارة الشبكات المطلوب لمديرية الأمن السيبراني و تكنولوجيا المعلومات :**
2. **SolarWinds System for Network 1**

|  |  |  |  |
| --- | --- | --- | --- |
| **No.** | **Item Name** | **Description** | **Qty.** |
| **Perpetual License with 1st-year Maintenance**  |
| 1. | NPM | SolarWinds Network Performance Monitor SL2000 (up to 2000 elements)  | 1 |
| 2. | NTA | SolarWinds NetFlow Traffic Analyzer Module for SolarWinds Network Performance Monitor SL2000 | 1 |
| 3. | NCM | SolarWinds Network Configuration Manager DL1000 (up to 1000 nodes) | 1 |
| 4. | NTM | SolarWinds Network Topology Mapper | 1 |
| **Annual Renewal (per year)**  |
| 1. | NPM | SolarWinds Network Performance Monitor SL2000 (up to 2000 elements)  | 2 |
| 2. | NTA | SolarWinds NetFlow Traffic Analyzer Module for SolarWinds Network Performance Monitor SL2000 | 2 |
| 3. | NCM | SolarWinds Network Configuration Manager DL1000 (up to 1000 nodes) | 2 |
| 4. | NTM | SolarWinds Network Topology Mapper | 2 |

1. **SolarWinds System for Network 2**

|  |  |  |  |
| --- | --- | --- | --- |
| **No.** | **Item Name** | **Description** | **Qty.** |
| **Perpetual License with 1st-year Maintenance**  |
| 1. | NPM | SolarWinds Network Performance Monitor SL2000 (up to 2000 elements)  | 1 |
| 2. | NTA | SolarWinds NetFlow Traffic Analyzer Module for SolarWinds Network Performance Monitor SL2000 | 1 |
| 3. | NCM | SolarWinds Network Configuration Manager DL500 (up to 500 nodes) | 1 |
| 4. | NTM | SolarWinds Network Topology Mapper | 1 |
| **Annual Renewal (per year)** |
| 1. | NPM | SolarWinds Network Performance Monitor SL2000 (up to 2000 elements)  | 2 |
| 2. | NTA | SolarWinds NetFlow Traffic Analyzer Module for SolarWinds Network Performance Monitor SL2000 | 2 |
| 3. | NCM | SolarWinds Network Configuration Manager DL500 (up to 500 nodes) | 2 |
| 4. | NTM | SolarWinds Network Topology Mapper | 2 |

1. **Abroad training**

|  |  |  |
| --- | --- | --- |
| **No.** | **Description** | **Qty.** |
| 1. | Solarwinds training: # 201 system management & monitoring.(Instructor-led training, 5 working day). | 4persons |

**ب. الشروط الخاصة:**

1. العطاء غير قابل للتجزئة.
2. مدة التسليم (6) أسابيع كحد أقصى.
3. العطاء شامل تنزيل الأنظمة وتشغيلها في مديرية الأمن السيبراني وتكنولوجيا المعلومات وكما يلي:
4. تنزيل الأنظمة على (Servers) موجودة على شبكات مديرية الأمن السيبراني وتكنولوجيا المعلومات.
5. الأنظمة المطلوبة عدد (2) لشبكات عدد (2) منفصلات عن بعضها (Two separated Networks)

جـ. الرخص السنوية المطلوبة والصيانة لمدة (3) عام.

1. شروط الدفع:
2. الدفعة الأولى عند الانتهاء من تشغيل الأنظمة وتفعيل الرخص عليها وتنفيذ التدريب المطلوب.
3. الدفعة الثانية في بداية العام الثاني مقابل تجديد الرخص لمدة عام.

جـ. الدفعة الثالثة في بداية العام الثالث مقابل تجديد الرخص لمدة عام.

1. الدورات شاملة كافة التكاليف من اقامة وتذاكر وتنقل ورسوم الدورة والتأشيرات وكل ما يلزم.
2. يجب الالتزام بكافة محتويات المواصفات والشروط.
3. العرض يجب ان يشمل ورقة مطابقة على شكل جدول يحتوي المواصفات المطلوبة والمواصفات المقدمة من الشركة وبالاشارة الى الكاتلوج الفني، عدم تقديم هذه الورقة يعطي الحق للجنة الشراء برفض العرض وتكون الشركة مسؤولة عن جميع المعلومات داخلها.