الكميات والمواصفات الفنية لمشروع نظام مراقبة الأثاث واللوازم.

|  |  |  |  |
| --- | --- | --- | --- |
| specs | QTY | Item | # |
| 4MP IR Fixed Bullet Network Camera, POE, 0.005 LUX, 30m IR distance, IP67, H.265+, H.264+H.264 Three streams. | 21 | Out door Fixed camera | 1 |
| 32 channel IP NVR, 4K resolution, management software with all required licenses ,Support 1-ch HDMI,1-ch VGA,HMDI at up to 4K (3840x2160) resolution, storage 4 TB included .  | 1 | NVR | 2 |
| 2 HDMI Port minimum, wall bracket. | 1 | 50 Inch monitor  | 3 |
| 20m. | 1 | HDMI Cable  | 4 |
| managed, POE, 8 10/100/1000Mbps RJ45 ports, 2Gigabit copper/SFP combo. | 5 | Network Switch  | 5 |
| Glass door, PDU and FAN. | 5 | Cabinet 6u. | 6 |
| Single mode Fiber 3m. | 6 | Fiber Patch cords. | 7 |
| 12 core Single mode Steel armored. | 800m | Fiber cable | 8 |
| UTP Cat6 cable(box 305m) | 3 box | UTP cable  | 9 |
| Fiber Patch Panel including connectors, couplers. Etc. | 2 | ODF 12 Core fully loaded | 10 |
| Fiber Patch Panel including connectors, couplers. Etc. | 2 | ODF 6 Core fully loaded | 11 |
| 1000 BASE-LH SFP( Transceiver for single mode fiber). | 6 | SFP SM . | 12 |
| 25\*20mm | 60m | Trunks | 13 |
| ـ ـ ـ ـ ـ | ـ ـ ـ ـ ـ | System Installation including( UTP and fiber pulling and termination, testing, operation, etc..).  | 14 |