|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **No.** | **Item Name** | **Description** | **Service Duration (Months)** | **Qty.** |
| **System for Network 1** | | | | |
| **1.0** | **PI-UCSM5-APL-K9** | **Cisco Prime Infrastructure UCS Physical HW Appliance (Gen 3)** | **-** | **1** |
| 1.0.1 | CON-SNT-PIUCSM5A | SNTC-8X5XNBD Cisco Prime Infrastructure UCS Physical | 36 | 1 |
| 1.1 | PI-HD12TB10K12N | 1.2 TB 12G SAS 10K RPM SFF HDD | - | 4 |
| 1.2 | PI-UCS-APL-IMG-3.6 | Cisco Prime Infrastructure 3.6 UCS Appliance Software | - | 1 |
| 1.3 | CAB-9K10A-UK | Power Cord, 250VAC 10A BS1363 Plug (13 A fuse), UK | - | 2 |
| 1.4 | PI-CPU-6148 | 2.4 GHz 6148/150W 20C/27.50MB Cache/DDR4 2666MHz | - | 1 |
| 1.5 | PI-MR-X16G1RS-H | 16GB DDR4-2666-MHz RDIMM/PC4-21300/single rank/x4/1.2v | - | 4 |
| 1.6 | PI-SD-32G-S | 32GB SD Card for UCS servers | - | 2 |
| 1.7 | PI-UCSC-PSU1-770W | 770W AC Hot-Plug Power Supply for 1U C-Series Rack Server | - | 2 |
| 1.8 | PI-MSTOR-SD | Mini Storage Carrier for SD (holds up to 2) | - | 1 |
| 1.9 | PI-RAID-M5 | Cisco 12G Modular RAID controller with 2GB cache | - | 1 |
| **2.0** | **R-MGMT3X-N-K9** | **Cisco Ent MGMT: Lic For Prime Infrastructure 3.x** | **-** | **1** |
| 2.0.1 | CON-ECMU-RMGMT3XN | SWSS UPGRADES Cisco MGMT: Lic For Prime Infra 3.x And | 36 | 1 |
| 2.1 | R-PI36-SW-K9 | Prime Infrastructure 3.6 Software | - | 1 |
| 2.2 | L-MGMT3X-PI-BASE | Cisco Ent MGMT: PI 3.x Platform Base Lic | - | 1 |
| 2.2.0.1 | CON-ECMU-LMGMBASE | SWSS UPGRADES Cisco Ent MGMT PI 3.x Platform Base Lic | 36 | 1 |
| 2.3 | L-MGMT3X-2K-K9 | Cisco Ent MGMT: PI 3.x LF,AS , 1 Cat 2K | - | 150 |
| 2.3.0.1 | CON-ECMU-LMGMT32X | SWSS UPGRADES Cisco Ent MGMT: PI 3 | 36 | 150 |
| 2.4 | L-MGMT3X-4K-K9 | Cisco Ent MGMT: PI 3.x LF,AS , 1 Cat 4K | - | 2 |
| 2.4.0.1 | CON-ECMU-LMGMT4KK | SWSS UPGRADES Cisco Ent MGMT:PI 3.x LF,AS APIC-EM L | 36 | 2 |
| 2.5 | L-MGMT3X-ISR1-K9 | Cisco Ent MGMT: PI 3.x LF, AS , 1 ISR1K | - | 90 |
| 2.5.0.1 | CON-ECMU-LMGMT3X9 | SWSS UPGRADES Cisco Ent MGMT: PI 3 | 36 | 90 |
| 2.6 | L-MGMT3X-ISR2-K9 | Cisco Ent MGMT: PI 3.x LF, AS , 1 ISR2K | - | 8 |
| 2.6.0.1 | CON-ECMU-LMGMT3KX | SWSS UPGRADES Cisco Ent MGMT: PI 3 | 36 | 8 |
| **System for Network 2** | | | | |
| **3.0** | **PI-UCSM5-APL-K9** | **Cisco Prime Infrastructure UCS Physical HW Appliance (Gen 3)** | **-** | **1** |
| 3.0.1 | CON-SNT-PIUCSM5A | SNTC-8X5XNBD Cisco Prime Infrastructure UCS Physical | 36 | 1 |
| 3.1 | PI-HD12TB10K12N | 1.2 TB 12G SAS 10K RPM SFF HDD | - | 4 |
| 3.2 | PI-UCS-APL-IMG-3.6 | Cisco Prime Infrastructure 3.6 UCS Appliance Software | - | 1 |
| 3.3 | CAB-9K10A-UK | Power Cord, 250VAC 10A BS1363 Plug (13 A fuse), UK | - | 2 |
| 3.4 | PI-CPU-6148 | 2.4 GHz 6148/150W 20C/27.50MB Cache/DDR4 2666MHz | - | 1 |
| 3.5 | PI-MR-X16G1RS-H | 16GB DDR4-2666-MHz RDIMM/PC4-21300/single rank/x4/1.2v | - | 4 |
| 3.6 | PI-SD-32G-S | 32GB SD Card for UCS servers | - | 2 |
| 3.7 | PI-UCSC-PSU1-770W | 770W AC Hot-Plug Power Supply for 1U C-Series Rack Server | - | 2 |
| 3.8 | PI-MSTOR-SD | Mini Storage Carrier for SD (holds up to 2) | - | 1 |
| 3.9 | PI-RAID-M5 | Cisco 12G Modular RAID controller with 2GB cache | - | 1 |
| **4.0** | **R-MGMT3X-N-K9** | **Cisco Ent MGMT: Lic For Prime Infrastructure 3.x** | **-** | **1** |
| 4.0.1 | CON-ECMU-RMGMT3XN | SWSS UPGRADES Cisco MGMT: Lic For Prime Infra 3.x And | 36 | 1 |
| 4.1 | R-PI36-SW-K9 | Prime Infrastructure 3.6 Software | - | 1 |
| 4.2 | L-MGMT3X-PI-BASE | Cisco Ent MGMT: PI 3.x Platform Base Lic | - | 1 |
| 4.2.0.1 | CON-ECMU-LMGMBASE | SWSS UPGRADES Cisco Ent MGMT PI 3.x Platform Base Lic | 36 | 1 |
| 4.3 | L-MGMT3X-2K-K9 | Cisco Ent MGMT: PI 3.x LF,AS , 1 Cat 2K | - | 150 |
| 4.3.0.1 | CON-ECMU-LMGMT32X | SWSS UPGRADES Cisco Ent MGMT: PI 3 | 36 | 150 |
| 4.4 | L-MGMT3X-4K-K9 | Cisco Ent MGMT: PI 3.x LF,AS , 1 Cat 4K | - | 4 |
| 4.4.0.1 | CON-ECMU-LMGMT4KK | SWSS UPGRADES Cisco Ent MGMT:PI 3.x LF,AS APIC-EM L | 36 | 4 |
| 4.5 | L-MGMT3X-ISR1-K9 | Cisco Ent MGMT: PI 3.x LF, AS , 1 ISR1K | - | 50 |
| 4.5.0.1 | CON-ECMU-LMGMT3X9 | SWSS UPGRADES Cisco Ent MGMT: PI 3 | 36 | 50 |
| 4.6 | L-MGMT3X-ASR1K9 | Cisco Ent MGMT: PI 3.x LF, AS , 1 ASR1K | - | 1 |
| 4.6.0.1 | CON-ECMU-LMGMTSR1 | SWSS UPGRADES Cisco Ent MGMTPI 3.x LF, AS APIC EM | 36 | 1 |
| **Abroad training** | | | | |
| 5.0 | MENPI | Managing Enterprise Networks with Cisco Prime Infrastructure | - | 4  person |

**الشروط الخاصة:**

1. العطاء غير قابل للتجزئة.
2. مدة التسليم (16) أسبوع كحد أقصى.
3. العطاء شامل التركيب والتشغيل في مديرية الأمن السيبراني و تكنولوجيا المعلومات.
4. الدورات شاملة كافة التكاليف من اقامة وتذاكر وتنقل ورسوم الدورة والتأشيرات وكل ما يلزم.
5. الدورات يجب أن تعقد حسب معايير (Cisco standard) من خلال مركز ومدرب معتمدين من شركة سيسكو (Cisco certified)
6. تقوم الشركة بالصاق (label) على الأجهزة يحتوي على اسم الشركة ورقم قرار الاحالة وتاريخ التوريد.
7. يجب الالتزام بكافة محتويات المواصفات والشروط.
8. العرض يجب ان يشمل ورقة مطابقة على شكل جدول يحتوي المواصفات المطلوبة والمواصفات المقدمة من الشركة وبالاشارة الى الكاتلوج الفني، عدم تقديم هذه الورقة يعطي الحق للجنة الشراء برفض العرض وتكون الشركة مسؤولة عن جميع المعلومات داخلها.